#MicroXplorer Configuration settings - do not modify
Dma.MEMTOMEM.10.Direction=DMA_MEMORY_TO_MEMORY
Dma.MEMTOMEM.10.FIFOMode=DMA_FIFOMODE_ENABLE
Dma.MEMTOMEM.10.FIFOThreshold=DMA_FIFO_THRESHOLD_FULL
Dma.MEMTOMEM.10.Instance=DMA2_Stream4
Dma.MEMTOMEM.10.MemBurst=DMA_MBURST_SINGLE
Dma.MEMTOMEM.10.MemDataAlignment=DMA_MDATAALIGN_WORD
Dma.MEMTOMEM.10.MemInc=DMA_MINC_DISABLE
Dma.MEMTOMEM.10.Mode=DMA_NORMAL
Dma.MEMTOMEM.10.PeriphBurst=DMA_PBURST_SINGLE
Dma.MEMTOMEM.10.PeriphDataAlignment=DMA_PDATAALIGN_WORD
Dma.MEMTOMEM.10.PeriphInc=DMA_PINC_ENABLE
Dma.MEMTOMEM.10.Priority=DMA_PRIORITY_LOW
Dma.MEMTOMEM.10.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode,FIFOThreshold,MemBurst,PeriphBurst
Dma.MEMTOMEM.11.Direction=DMA_MEMORY_TO_MEMORY
Dma.MEMTOMEM.11.FIFOMode=DMA_FIFOMODE_ENABLE
Dma.MEMTOMEM.11.FIFOThreshold=DMA_FIFO_THRESHOLD_FULL
Dma.MEMTOMEM.11.Instance=DMA2_Stream3
Dma.MEMTOMEM.11.MemBurst=DMA_MBURST_SINGLE
Dma.MEMTOMEM.11.MemDataAlignment=DMA_MDATAALIGN_WORD
Dma.MEMTOMEM.11.MemInc=DMA_MINC_ENABLE
Dma.MEMTOMEM.11.Mode=DMA_NORMAL
Dma.MEMTOMEM.11.PeriphBurst=DMA_PBURST_SINGLE
Dma.MEMTOMEM.11.PeriphDataAlignment=DMA_PDATAALIGN_WORD
Dma.MEMTOMEM.11.PeriphInc=DMA_PINC_ENABLE
Dma.MEMTOMEM.11.Priority=DMA_PRIORITY_LOW
Dma.MEMTOMEM.11.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode,FIFOThreshold,MemBurst,PeriphBurst
Dma.Request0=USART6_RX
Dma.Request1=USART6_TX
Dma.Request10=MEMTOMEM
Dma.Request11=MEMTOMEM
Dma.Request2=USART1_RX
Dma.Request3=USART1_TX
Dma.Request4=USART2_RX
Dma.Request5=USART2_TX
Dma.Request6=USART3_RX
Dma.Request7=USART3_TX
Dma.Request8=UART4_RX
Dma.Request9=UART4_TX
Dma.RequestsNb=12
Dma.UART4_RX.8.Direction=DMA_PERIPH_TO_MEMORY
Dma.UART4_RX.8.FIFOMode=DMA_FIFOMODE_DISABLE
Dma.UART4_RX.8.Instance=DMA1_Stream2
Dma.UART4_RX.8.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.UART4_RX.8.MemInc=DMA_MINC_ENABLE
Dma.UART4_RX.8.Mode=DMA_NORMAL
Dma.UART4_RX.8.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.UART4_RX.8.PeriphInc=DMA_PINC_DISABLE
Dma.UART4_RX.8.Priority=DMA_PRIORITY_LOW
Dma.UART4_RX.8.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode
Dma.UART4_TX.9.Direction=DMA_MEMORY_TO_PERIPH
Dma.UART4_TX.9.FIFOMode=DMA_FIFOMODE_DISABLE
Dma.UART4_TX.9.Instance=DMA1_Stream4
Dma.UART4_TX.9.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.UART4_TX.9.MemInc=DMA_MINC_ENABLE
Dma.UART4_TX.9.Mode=DMA_NORMAL
Dma.UART4_TX.9.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.UART4_TX.9.PeriphInc=DMA_PINC_DISABLE
Dma.UART4_TX.9.Priority=DMA_PRIORITY_LOW
Dma.UART4_TX.9.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode
Dma.USART1_RX.2.Direction=DMA_PERIPH_TO_MEMORY
Dma.USART1_RX.2.FIFOMode=DMA_FIFOMODE_DISABLE
Dma.USART1_RX.2.Instance=DMA2_Stream2
Dma.USART1_RX.2.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.USART1_RX.2.MemInc=DMA_MINC_ENABLE
Dma.USART1_RX.2.Mode=DMA_NORMAL
Dma.USART1_RX.2.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.USART1_RX.2.PeriphInc=DMA_PINC_DISABLE
Dma.USART1_RX.2.Priority=DMA_PRIORITY_MEDIUM
Dma.USART1_RX.2.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode
Dma.USART1_TX.3.Direction=DMA_MEMORY_TO_PERIPH
Dma.USART1_TX.3.FIFOMode=DMA_FIFOMODE_DISABLE
Dma.USART1_TX.3.Instance=DMA2_Stream7
Dma.USART1_TX.3.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.USART1_TX.3.MemInc=DMA_MINC_ENABLE
Dma.USART1_TX.3.Mode=DMA_NORMAL
Dma.USART1_TX.3.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.USART1_TX.3.PeriphInc=DMA_PINC_DISABLE
Dma.USART1_TX.3.Priority=DMA_PRIORITY_MEDIUM
Dma.USART1_TX.3.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode
Dma.USART2_RX.4.Direction=DMA_PERIPH_TO_MEMORY
Dma.USART2_RX.4.FIFOMode=DMA_FIFOMODE_DISABLE
Dma.USART2_RX.4.Instance=DMA1_Stream5
Dma.USART2_RX.4.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.USART2_RX.4.MemInc=DMA_MINC_ENABLE
Dma.USART2_RX.4.Mode=DMA_NORMAL
Dma.USART2_RX.4.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.USART2_RX.4.PeriphInc=DMA_PINC_DISABLE
Dma.USART2_RX.4.Priority=DMA_PRIORITY_MEDIUM
Dma.USART2_RX.4.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode
Dma.USART2_TX.5.Direction=DMA_MEMORY_TO_PERIPH
Dma.USART2_TX.5.FIFOMode=DMA_FIFOMODE_DISABLE
Dma.USART2_TX.5.Instance=DMA1_Stream6
Dma.USART2_TX.5.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.USART2_TX.5.MemInc=DMA_MINC_ENABLE
Dma.USART2_TX.5.Mode=DMA_NORMAL
Dma.USART2_TX.5.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.USART2_TX.5.PeriphInc=DMA_PINC_DISABLE
Dma.USART2_TX.5.Priority=DMA_PRIORITY_MEDIUM
Dma.USART2_TX.5.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode
Dma.USART3_RX.6.Direction=DMA_PERIPH_TO_MEMORY
Dma.USART3_RX.6.FIFOMode=DMA_FIFOMODE_DISABLE
Dma.USART3_RX.6.Instance=DMA1_Stream1
Dma.USART3_RX.6.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.USART3_RX.6.MemInc=DMA_MINC_ENABLE
Dma.USART3_RX.6.Mode=DMA_NORMAL
Dma.USART3_RX.6.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.USART3_RX.6.PeriphInc=DMA_PINC_DISABLE
Dma.USART3_RX.6.Priority=DMA_PRIORITY_MEDIUM
Dma.USART3_RX.6.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode
Dma.USART3_TX.7.Direction=DMA_MEMORY_TO_PERIPH
Dma.USART3_TX.7.FIFOMode=DMA_FIFOMODE_DISABLE
Dma.USART3_TX.7.Instance=DMA1_Stream3
Dma.USART3_TX.7.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.USART3_TX.7.MemInc=DMA_MINC_ENABLE
Dma.USART3_TX.7.Mode=DMA_NORMAL
Dma.USART3_TX.7.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.USART3_TX.7.PeriphInc=DMA_PINC_DISABLE
Dma.USART3_TX.7.Priority=DMA_PRIORITY_MEDIUM
Dma.USART3_TX.7.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode
Dma.USART6_RX.0.Direction=DMA_PERIPH_TO_MEMORY
Dma.USART6_RX.0.FIFOMode=DMA_FIFOMODE_DISABLE
Dma.USART6_RX.0.Instance=DMA2_Stream1
Dma.USART6_RX.0.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.USART6_RX.0.MemInc=DMA_MINC_ENABLE
Dma.USART6_RX.0.Mode=DMA_NORMAL
Dma.USART6_RX.0.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.USART6_RX.0.PeriphInc=DMA_PINC_DISABLE
Dma.USART6_RX.0.Priority=DMA_PRIORITY_MEDIUM
Dma.USART6_RX.0.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode
Dma.USART6_TX.1.Direction=DMA_MEMORY_TO_PERIPH
Dma.USART6_TX.1.FIFOMode=DMA_FIFOMODE_DISABLE
Dma.USART6_TX.1.Instance=DMA2_Stream6
Dma.USART6_TX.1.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.USART6_TX.1.MemInc=DMA_MINC_ENABLE
Dma.USART6_TX.1.Mode=DMA_NORMAL
Dma.USART6_TX.1.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.USART6_TX.1.PeriphInc=DMA_PINC_DISABLE
Dma.USART6_TX.1.Priority=DMA_PRIORITY_MEDIUM
Dma.USART6_TX.1.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode
File.Version=6
KeepUserPlacement=false
Mcu.Family=STM32F4
Mcu.IP0=CRC
Mcu.IP1=DMA
Mcu.IP2=NVIC
Mcu.IP3=RCC
Mcu.IP4=SYS
Mcu.IP5=UART4
Mcu.IP6=USART1
Mcu.IP7=USART2
Mcu.IP8=USART3
Mcu.IP9=USART6
Mcu.IPNb=10
Mcu.Name=STM32F407V(E-G)Tx
Mcu.Package=LQFP100
Mcu.Pin0=PE3
Mcu.Pin1=PE4
Mcu.Pin10=PA0-WKUP
Mcu.Pin11=PA1
Mcu.Pin12=PA2
Mcu.Pin13=PA3
Mcu.Pin14=PA6
Mcu.Pin15=PA7
Mcu.Pin16=PB10
Mcu.Pin17=PB11
Mcu.Pin18=PC6
Mcu.Pin19=PC7
Mcu.Pin2=PC14-OSC32_IN
Mcu.Pin20=PA9
Mcu.Pin21=PA10
Mcu.Pin22=PA13
Mcu.Pin23=PA14
Mcu.Pin24=PB3
Mcu.Pin25=VP_CRC_VS_CRC
Mcu.Pin26=VP_SYS_VS_Systick
Mcu.Pin3=PC15-OSC32_OUT
Mcu.Pin4=PH0-OSC_IN
Mcu.Pin5=PH1-OSC_OUT
Mcu.Pin6=PC0
Mcu.Pin7=PC1
Mcu.Pin8=PC2
Mcu.Pin9=PC3
Mcu.PinsNb=27
Mcu.ThirdPartyNb=0
Mcu.UserConstants=
Mcu.UserName=STM32F407VETx
MxCube.Version=5.4.0
MxDb.Version=DB.5.0.40
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.DMA1_Stream1_IRQn=true\:1\:0\:true\:false\:true\:false\:true
NVIC.DMA1_Stream2_IRQn=true\:1\:0\:true\:false\:true\:false\:true
NVIC.DMA1_Stream3_IRQn=true\:1\:0\:true\:false\:true\:false\:true
NVIC.DMA1_Stream4_IRQn=true\:1\:0\:true\:false\:true\:false\:true
NVIC.DMA1_Stream5_IRQn=true\:1\:0\:true\:false\:true\:false\:true
NVIC.DMA1_Stream6_IRQn=true\:1\:0\:true\:false\:true\:false\:true
NVIC.DMA2_Stream1_IRQn=true\:1\:0\:true\:false\:true\:false\:true
NVIC.DMA2_Stream2_IRQn=true\:1\:0\:true\:false\:true\:false\:true
NVIC.DMA2_Stream3_IRQn=true\:0\:0\:false\:false\:true\:true\:true
NVIC.DMA2_Stream4_IRQn=true\:0\:0\:false\:false\:true\:true\:true
NVIC.DMA2_Stream6_IRQn=true\:1\:0\:true\:false\:true\:false\:true
NVIC.DMA2_Stream7_IRQn=true\:1\:0\:true\:false\:true\:false\:true
NVIC.DebugMonitor_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.ForceEnableDMAVector=true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.PendSV_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.SysTick_IRQn=true\:0\:0\:false\:false\:true\:false\:true
NVIC.UART4_IRQn=true\:1\:0\:true\:false\:true\:true\:true
NVIC.USART1_IRQn=true\:1\:0\:true\:false\:true\:true\:true
NVIC.USART2_IRQn=true\:1\:0\:true\:false\:true\:true\:true
NVIC.USART3_IRQn=true\:1\:0\:true\:false\:true\:true\:true
NVIC.USART6_IRQn=true\:1\:0\:true\:false\:true\:true\:true
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false
PA0-WKUP.Mode=Asynchronous
PA0-WKUP.Signal=UART4_TX
PA1.Mode=Asynchronous
PA1.Signal=UART4_RX
PA10.Mode=Asynchronous
PA10.Signal=USART1_RX
PA13.Mode=Trace_Asynchronous_SW
PA13.Signal=SYS_JTMS-SWDIO
PA14.Mode=Trace_Asynchronous_SW
PA14.Signal=SYS_JTCK-SWCLK
PA2.Mode=Asynchronous
PA2.Signal=USART2_TX
PA3.Mode=Asynchronous
PA3.Signal=USART2_RX
PA6.GPIOParameters=GPIO_Label
PA6.GPIO_Label=LED0
PA6.Locked=true
PA6.Signal=GPIO_Output
PA7.GPIOParameters=GPIO_Label
PA7.GPIO_Label=LED1
PA7.Locked=true
PA7.Signal=GPIO_Output
PA9.Mode=Asynchronous
PA9.Signal=USART1_TX
PB10.Mode=Asynchronous
PB10.Signal=USART3_TX
PB11.Mode=Asynchronous
PB11.Signal=USART3_RX
PB3.Mode=Trace_Asynchronous_SW
PB3.Signal=SYS_JTDO-SWO
PC0.GPIOParameters=GPIO_Label
PC0.GPIO_Label=DBG0
PC0.Locked=true
PC0.Signal=GPIO_Output
PC1.GPIOParameters=GPIO_Label
PC1.GPIO_Label=DBG1
PC1.Locked=true
PC1.Signal=GPIO_Output
PC14-OSC32_IN.Mode=LSE-External-Oscillator
PC14-OSC32_IN.Signal=RCC_OSC32_IN
PC15-OSC32_OUT.Mode=LSE-External-Oscillator
PC15-OSC32_OUT.Signal=RCC_OSC32_OUT
PC2.GPIOParameters=GPIO_Label
PC2.GPIO_Label=DBG2
PC2.Locked=true
PC2.Signal=GPIO_Output
PC3.GPIOParameters=GPIO_Label
PC3.GPIO_Label=DBG3
PC3.Locked=true
PC3.Signal=GPIO_Output
PC6.Mode=Asynchronous
PC6.Signal=USART6_TX
PC7.Mode=Asynchronous
PC7.Signal=USART6_RX
PCC.Checker=false
PCC.Line=STM32F407/417
PCC.MCU=STM32F407V(E-G)Tx
PCC.PartNumber=STM32F407VETx
PCC.Seq0=0
PCC.Series=STM32F4
PCC.Temperature=25
PCC.Vdd=3.3
PE3.GPIOParameters=GPIO_PuPd,GPIO_Label
PE3.GPIO_Label=KEY1
PE3.GPIO_PuPd=GPIO_PULLUP
PE3.Locked=true
PE3.Signal=GPIO_Input
PE4.GPIOParameters=GPIO_PuPd,GPIO_Label
PE4.GPIO_Label=KEY0
PE4.GPIO_PuPd=GPIO_PULLUP
PE4.Locked=true
PE4.Signal=GPIO_Input
PH0-OSC_IN.Mode=HSE-External-Oscillator
PH0-OSC_IN.Signal=RCC_OSC_IN
PH1-OSC_OUT.Mode=HSE-External-Oscillator
PH1-OSC_OUT.Signal=RCC_OSC_OUT
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=true
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=true
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32F407VETx
ProjectManager.FirmwarePackage=STM32Cube FW_F4 V1.24.1
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0x200
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=1
ProjectManager.MainLocation=Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=STM32CubeIDE
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=mississippi-mcu-packetusart-testbed.ioc
ProjectManager.ProjectName=mississippi-mcu-packetusart-testbed
ProjectManager.StackSize=0x400
ProjectManager.TargetToolchain=STM32CubeIDE
ProjectManager.ToolChainLocation=
ProjectManager.UnderRoot=true
ProjectManager.functionlistsort=1-MX_GPIO_Init-GPIO-false-LL-true,2-MX_DMA_Init-DMA-false-LL-true,3-SystemClock_Config-RCC-false-HAL-false,4-MX_UART4_Init-UART4-false-LL-true,5-MX_USART1_UART_Init-USART1-false-LL-true,6-MX_USART2_UART_Init-USART2-false-LL-true,7-MX_USART3_UART_Init-USART3-false-LL-true,8-MX_USART6_UART_Init-USART6-false-LL-true,9-MX_CRC_Init-CRC-false-LL-true
RCC.48MHZClocksFreq_Value=84000000
RCC.AHBFreq_Value=168000000
RCC.APB1CLKDivider=RCC_HCLK_DIV4
RCC.APB1Freq_Value=42000000
RCC.APB1TimFreq_Value=84000000
RCC.APB2CLKDivider=RCC_HCLK_DIV2
RCC.APB2Freq_Value=84000000
RCC.APB2TimFreq_Value=168000000
RCC.CortexFreq_Value=168000000
RCC.EthernetFreq_Value=168000000
RCC.FCLKCortexFreq_Value=168000000
RCC.FLatency=FLASH_LATENCY_5
RCC.FamilyName=M
RCC.HCLKFreq_Value=168000000
RCC.HSE_VALUE=25000000
RCC.HSI_VALUE=16000000
RCC.I2SClocksFreq_Value=192000000
RCC.IPParameters=48MHZClocksFreq_Value,AHBFreq_Value,APB1CLKDivider,APB1Freq_Value,APB1TimFreq_Value,APB2CLKDivider,APB2Freq_Value,APB2TimFreq_Value,CortexFreq_Value,EthernetFreq_Value,FCLKCortexFreq_Value,FLatency,FamilyName,HCLKFreq_Value,HSE_VALUE,HSI_VALUE,I2SClocksFreq_Value,LSI_VALUE,MCO2PinFreq_Value,PLLCLKFreq_Value,PLLM,PLLN,PLLQCLKFreq_Value,RTCFreq_Value,RTCHSEDivFreq_Value,SYSCLKFreq_VALUE,SYSCLKSource,VCOI2SOutputFreq_Value,VCOInputFreq_Value,VCOOutputFreq_Value,VcooutputI2S
RCC.LSI_VALUE=32000
RCC.MCO2PinFreq_Value=168000000
RCC.PLLCLKFreq_Value=168000000
RCC.PLLM=8
RCC.PLLN=168
RCC.PLLQCLKFreq_Value=84000000
RCC.RTCFreq_Value=32000
RCC.RTCHSEDivFreq_Value=12500000
RCC.SYSCLKFreq_VALUE=168000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.VCOI2SOutputFreq_Value=384000000
RCC.VCOInputFreq_Value=2000000
RCC.VCOOutputFreq_Value=336000000
RCC.VcooutputI2S=192000000
UART4.BaudRate=115200
UART4.IPParameters=BaudRate,WordLength,Parity,StopBits,Mode,OverSampling,VirtualMode
UART4.Mode=MODE_TX_RX
UART4.OverSampling=UART_OVERSAMPLING_16
UART4.Parity=PARITY_NONE
UART4.StopBits=UART_STOPBITS_1
UART4.VirtualMode=Asynchronous
UART4.WordLength=WORDLENGTH_8B
USART1.BaudRate=5250000
USART1.IPParameters=BaudRate,WordLength,Parity,StopBits,Mode,OverSampling,VirtualMode
USART1.Mode=MODE_TX_RX
USART1.OverSampling=UART_OVERSAMPLING_16
USART1.Parity=PARITY_NONE
USART1.StopBits=STOPBITS_1
USART1.VirtualMode=VM_ASYNC
USART1.WordLength=WORDLENGTH_8B
USART2.BaudRate=5250000
USART2.IPParameters=BaudRate,WordLength,Parity,StopBits,Mode,OverSampling,VirtualMode
USART2.Mode=MODE_TX_RX
USART2.OverSampling=UART_OVERSAMPLING_8
USART2.Parity=PARITY_NONE
USART2.StopBits=STOPBITS_1
USART2.VirtualMode=VM_ASYNC
USART2.WordLength=WORDLENGTH_8B
USART3.BaudRate=5250000
USART3.IPParameters=BaudRate,WordLength,Parity,StopBits,Mode,OverSampling,VirtualMode
USART3.Mode=MODE_TX_RX
USART3.OverSampling=UART_OVERSAMPLING_8
USART3.Parity=PARITY_NONE
USART3.StopBits=STOPBITS_1
USART3.VirtualMode=VM_ASYNC
USART3.WordLength=WORDLENGTH_8B
USART6.BaudRate=5250000
USART6.IPParameters=BaudRate,WordLength,Parity,StopBits,Mode,OverSampling,VirtualMode
USART6.Mode=MODE_TX_RX
USART6.OverSampling=UART_OVERSAMPLING_16
USART6.Parity=PARITY_NONE
USART6.StopBits=STOPBITS_1
USART6.VirtualMode=VM_ASYNC
USART6.WordLength=WORDLENGTH_8B
VP_CRC_VS_CRC.Mode=CRC_Activate
VP_CRC_VS_CRC.Signal=CRC_VS_CRC
VP_SYS_VS_Systick.Mode=SysTick
VP_SYS_VS_Systick.Signal=SYS_VS_Systick
board=custom
